**H168N WirelessVDSL2 Uplink Gateway**

H168N is a Wireless and VDSL2 uplink gateway. Comprehensive QoS techniques ensure the simultaneous use of services with a good level of performance. DLNA server enables multimedia contents sharing. The integration of TR-069 technologies facilitates the automatic installation and the automatic provisioning of services.

 http://wwwen.zte.com.cn/en/products/access/cpe/201405/W020140522395882921148.gifhttp://wwwen.zte.com.cn/en/products/access/cpe/201405/W020140522395882994819.gifhttp://wwwen.zte.com.cn/en/products/access/cpe/201405/W020140522395883063432.gifhttp://wwwen.zte.com.cn/en/products/access/cpe/201405/W020140522395883140709.gifhttp://wwwen.zte.com.cn/en/products/access/cpe/201405/W020140522395883211215.gifhttp://wwwen.zte.com.cn/en/products/access/cpe/201405/W020140522395883288246.gif

wifi.pngDLNA.png

**Features**

* VDSL wireless modem
* Multimode VDSL2 (up to 17a profile) / ADSL2+
* G.Vector+G.INP to maximize data rate of VDSL
* Dual-Stream 802.11n Wi-Fi up to 300Mbps
* Fast Ethernet 4-port switch
* USB 2.0 for shared storage or 3G Dongle
* Built-in DLNA Digital Media Server
* Robust remote management - TR069
* IPv4/IPv6 Dual Stack and DS-Lite
* CoC Tier 2013-2014

**Specifications**

|  |  |  |
| --- | --- | --- |
| Physical Interface | WAN | VDSL2 / ADSL2+ |
| LAN | 4 x 10/100M FE  802.11b/g/n Wi-Fi @ 2.4G(2x2)  1 x USB 2.0 Host |
| Power Consumption | < 10W | |
| Net Weight | 190g | |
| Dimensions(L×W×H) | 146mm×54mm×126mm | |
| Operating Temperature | 0～40℃（32℉～104℉） | |
| Humidity | 5% - 95% | |