**H168N WirelessVDSL2 Uplink Gateway**

H168N is a Wireless and VDSL2 uplink gateway. Comprehensive QoS techniques ensure the simultaneous use of services with a good level of performance. DLNA server enables multimedia contents sharing. The integration of TR-069 technologies facilitates the automatic installation and the automatic provisioning of services.

 



 **Features**

* VDSL wireless modem
* Multimode VDSL2 (up to 17a profile) / ADSL2+
* G.Vector+G.INP to maximize data rate of VDSL
* Dual-Stream 802.11n Wi-Fi up to 300Mbps
* Fast Ethernet 4-port switch
* USB 2.0 for shared storage or 3G Dongle
* Built-in DLNA Digital Media Server
* Robust remote management - TR069
* IPv4/IPv6 Dual Stack and DS-Lite
* CoC Tier 2013-2014

 **Specifications**

|  |  |  |
| --- | --- | --- |
| Physical Interface  | WAN  | VDSL2 / ADSL2+  |
| LAN  | 4 x 10/100M FE802.11b/g/n Wi-Fi @ 2.4G(2x2)1 x USB 2.0 Host  |
| Power Consumption  | < 10W   |
| Net Weight  | 190g   |
| Dimensions(L×W×H)  | 146mm×54mm×126mm   |
| Operating Temperature  | 0～40℃（32℉～104℉）  |
| Humidity  | 5% - 95%  |